Summit 24 PIN Connector List (HMS.COM/SLOT_MACHINES/24 PIN CONNECTOR.rtf)
24 PIN FEMALE CONNECTOR (VIEW FROM FRONT) (NOT THE WIRE SIDE)
22   19   16   13   10   7   4   1 <- (TOP RIGHT)
23   20   17   14   11   8   5   2
24   21   18   15   12   9   6   3
PIN	WIRE COLOR	DESIGNATION
1	ORN/GRN	JP BELL/TOWER 
2	BRN/RED	DOOR HINGE SWITCH
3	BRN/BLK	JACK POT LIGHT (TOWER LIGHT)
4	UNUSED
5	BLK/RED	DC GROUND (OV DC)
6	BRN/BLU	COIN-OUT SWITCH (FROM HOPPER)
7	YEL		6 VAC/50VAC COMMON
8	BLU		6VAC HOT
9	GRY/YEL	HANDLE RELEASE
10	BLK/RED	DC GROUND (0V DC)
11	VIO (UNUSED)
12	WHT/BLK	HOPPER RUN (120 VAC WHEN HOPPER IS ENERGIZED)
13	WHT/GRY	HOPPER SAFE (120 VAC 'PULSED' WHEN HOPPER IS ENERGIZED)
14	BRN/ORN	UNUSED (TXD)
15	GRY		UNUSED (RXD)
16	UNUSED
17	WHT		120VAC COMMON
18	BLK		120VAC HOT
19	ORN		+5VDC
20	UNUSED
21	RED		50VAC HOT
22	GRN/WHT	UNUSED
23	UNUSED
24	BRN/GRN	J/P RESET SWITCH (SWITCH ON SIDE OF MACHINE)